**SecuRemote® Smart**

**Quick Start Guide**

**Keeler 3.0**

Version 01.01.04

Table of Contents

[1 Downloading and Installing SecuRemote® Smart Application from Store 3](#_Toc430894911)

[2 Installing SR Device 4](#_Toc430894912)

[3 Pairing with Keeler Lock 3.0 as First user-Admin 5](#_Toc430894913)

[4 Operate SR Device 6](#_Toc430894914)

[5 Add New User Access Device 7](#_Toc430894915)

[6 Invited User Device redeem “Invite Code” and pair with SR Device 8](#_Toc430894916)

[7 Register and Configure SR Bridge to UDI Portal 9](#_Toc430894917)

# Downloading and Installing SecuRemote® Smart Application from Store

Download & Install SR Smart or SecuRemote® Smart application from Apple app store or Google play store.

**For iPhone:**

* + Go to App Store in mobile device
  + Search for “SecuRemote” or “SecuRemote Smart” application
  + Install “SecuRemote® Smart” Application
  + You can directly open below link on your iPhone

<https://itunes.apple.com/us/app/securemote-smart/id967169177?mt=8>

**For Android:**

* Go to Play Store in mobile device
* Search for “SecuRemote” or “SecuRemote Smart” application
* Install “SecuRemote® Smart” Application
* You can directly open below link on your Android Phone

[https://play.google.com/store/apps/details?id=com.belwith.securemotesmart](https://play.google.com/store/apps/details?id=com.belwith.securemotesmartapp)

**Application icon or logo:**



# Installing SR Device

Refer to the SecuRemote Enabled Lock Installation Instructions which were included with your lock.

# Pairing with Keeler Lock 3.0 as First user-Admin

1. Click on the SR Smart app icon. The SR Smart app will be launched and the “Add SR Device” screen will appear.
2. User can either select “SCAN QR CODE” option or “Enter SR # manually” option.

* To add SR Device using “SCAN QR CODE”

#### Click on “SCAN QR CODE” button

#### SR Device info will be read successfully from label on Keeler, using QR scan.

##### Screen will appear with auto-filled SR device information.

##### User must enter a desired name for this SR Device and click on “Create New Account” Button

* To add SR Device using “SR # manually” option:

#### Click on “Enter SR # manually” from “Add SR Device” screen.

#### Enter SR # and Security Token from label attached to SR Device manually in “Add SR Device” screen.

* + User must enter a desired name for this SR Device and click on “Create New Account” Button

#### Click on “Create New Account” Button. “Create SR Account” screen will appear. User must provide email address and password to create a new account on the SR Portal. Enter all necessary account information, and click on “Register SR Device”.

#### SR Smart app will send SR Device information to the SRP for creating a new account and registering SR Device. SR Smart app will initiate the process and display a toast message “Registering SR Device…”

1. After registering your SR Device on SRP, the SR Device’s home screen will appear with various options.
2. For future reference, place a copy of the QR CODE and Serial Number on the inside, back cover of the SecuRemote Enabled Lock Installation Instructions manual, and keep the manual in a safe place. **Important: the last user to scan or enter the information into the SR Smart app is the Administrator.**

# Operate SR Device

* **In Local Mode**
  + - Make sure your mobile device Bluetooth is turned ON, the SR device is powered ON, and that both devices are within direct operation range.
    - Press Lock/Unlock from the Home Screen to operate the Keeler Lock.
* **In Remote Mode** 
  + - If your mobile device is not in direct range with the Keeler Lock, Lock or Unlock operation will be performed via Remote Mode.
    - Make sure the Keeler Lock is assigned to an SR Bridge on the SecuRemote Portal. (See **Register and Configure SR Bridge to UDI Portal** for detail)
    - Press Lock/Unlock from the Home Screen. It will ask to confirm remote operation. Tap on “Yes” to operate.

# Add New User Access Device

Internet connectivity is necessary to add a new user for the Keeler Lock.

* Launch the SR App and select Users🡪Invite Access Device.
* Admin will be asked to enter Email Id and Password of account and User name of invitee user.
* Click on “Get Invite Code” button
* With successful credentials, Admin will receive an INVITE CODE and can send it to user by SMS or by EMAIL.

**Note:** Invite Code can be used only once. In order to register user device again, a new invite code is required.

# Invited User Device redeem “Invite Code” and pair with SR Device

Invited user will need to download and install the SR Smart App from their App Store. Then the user will:

* Launch SR Smart App
* Add SR Device screen will appear
* Press on “Enter Invite Code” button
* Accept Invitation screen will appear
* Enter Invite Code that is received by SMS or EMAIL and press “Accept Invitation” button
* App will authenticate the invite code with SRP and display toast message “Validating Invitation Code…” during process of authentication.
* On successful authorization with SRP application, it will redirect to SR Device’s Home screen.

Now user can operate Keeler Lock in local mode using Bluetooth as well as remotely (if it is assigned to an SR Bridge).

# Register and Configure SR Bridge to UDI Portal

* Login to SecuRemote® Portal [http://portal.securemote.com](http://portal.securemote.com/) with the credentials that had been used while creating account.
* Go to “Bridges” tab. It will display SR Bridge list.
* Click on “Add Bridge” if you have not added a bridge device yet. Otherwise choose from the list in case you have added one from the mobile device app.
* Click on Bridge name under which SR Device will be assigned.
* Click on “Assign SecuRemote Device”. Select SR Device that has to be assigned under that SR Bridge.