|  |
| --- |
|  |
| SecuRemote Smart Release Notes – iOS App |
| Version 01.01.05 |



**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Version #** | **Remark** | **Date** | **Done By** |
| 01.01.05 | Release notes details of iOS app version 01.01.05 | 09/07/15 | Paresh |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

Table of Contents

1. Introduction 4

2. Definition(s) and Abbreviation(s) 5

3. App Version Details and Documents 6

4. Supported SR Devices 7

5. Release Features 8

5.1. Remember Me Option 8

5.2. Confirm Password 8

5.3. Device Log 8

5.4. Initial Padlock support 8

6. Enhancements 9

6.1. Settings Screen Flow 9

6.2. Guest User rights 9

6.3. Remove Admin PIN 9

6.4. Device Diagnostics for GDO 9

6.5. Firmware Upgrade as new SDK 07.02 9

7. Bug Fixes 10

7.1. Bug # 1890 10

7.2. Bug # 1869 10

7.3. Bug # 1816 10

7.4. Bug # 1750 10

7.5. Bug # 1721 10

7.6. Bug # 1685 10

7.7. Bug # 1547 10

8. Known Issues and Problems 11

8.1. Issue # 1 11

8.2. Issue # 2 11

8.3. Issue # 3 11

# Introduction

This document provides overview of the SR Smart mobile application new features, enhancements, bug fixes and performance improvements.

# Definition(s) and Abbreviation(s)

|  |  |
| --- | --- |
| **Name** | **Abbreviation** |
| SRP | SecuRemote online portal |
| SR Smart | SecuRemote Smart |
| SR Device | SecuRemote Device |
| Dev-Kit | SecuRemote Development Kit |
| App Version | It is displayed in Home Screen of SR Smart App |
| Build Version | It is displayed in Help Section |

# App Version Details and Documents

|  |  |
| --- | --- |
| **Name** | **Description** |
| Release Date | 08/07/2015 |
| App Version | 01.01.05 |
| Build Version | 01.01.41 |
| Help Version | 01.01.08 – [SR Smart Help Document](https://github.com/DelphianSystems/SecuRemote/blob/master/SR%20Smart%20Help/) |
| Requirement Document | 01.01.03 – [SR Smart Requirement Document](https://github.com/DelphianSystems/SecuRemote/blob/master/SR%20Smart%20App/) |
| User Manual | [SR Devices User Manuals Documents](https://github.com/DelphianSystems/SecuRemote/blob/master/User%20Manual/) |
| Quick Start Guide | [Quick Start Guide Documents](https://github.com/DelphianSystems/SecuRemote/blob/master/Quick%20Start%20Guide/) |
| IOS Compatibility | IOS 7.0 and above for all devices (iPhone, iPod Touch and iPad) having BLE support. It is optimized for iPhone 5, iPhone 6 and iPhone 6 Plus. It supports only portrait orientation. |
| IOS App URL | <https://itunes.apple.com/us/app/securemote-smart/id967169177?mt=8> |
| Language | English |

# Supported SR Devices

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Name** | **Description of supported versions** | | | | | | | |
| RAS 2.0(Smart Deadbolt) | BLE App firmware version | | BLE Boot loader version | | | | Hardware version | |
| 05.01.01 with EPROM | | 01.01.02 with EPROM | | | | 03.03.02 with EPROM | |
| 04.01.08 without EPROM | | 01.01.01 without EPROM | | | | 03.01.03 without EPROM | |
| Keeler | BLE App firmware version | BLE Boot loader version | | BLE Soft device version | | MSP430 (Audio) version | | Hardware version |
| 02.01.03 | 01.01.02 | | S310 v01.00.00 | | 02.01.02 | | 01.02.03 |
| GDO | BLE Controller (BLE) | | Nordic Controller (NWC) | | | | Hardware version | |
| 01.01.12 | | 02.01.03 | | | | 01.01.04 | |
| SR Bridge | BLE Controller (BLE) | | | | Nordic Controller (NWC) | | | |
| 01.01.02 | | | | 02.01.03 | | | |
| Keyfob | Keyfob (02.01.09) | | | | | | | |
| SR Development Kit | Dev-kit (04.01.05) | | | | | | | |

# Release Features

## Remember Me Option

This feature will save user’s email id and password. It will not ask user again until log out from the app.

## Confirm Password

This feature will ask user to verify password entered. It will make sure user has typed the correct password as per choice. It will be verify with confirm password field next to actual password field.

## Device Log

This feature will allow user to send mobile device log to developer team. Developer can easily debug the issue by verifying the log and provide solution to user.

## Initial Padlock support

This feature will allow user to add Padlock device and perform its operations and features.

# Enhancements

## Settings Screen Flow

User will have separate settings for SR Device, App Settings. Audit Trail, Delete SR Device, Log out options is added in the settings screen separately.

## Guest User rights

Guest user is also can perform any admin task if having correct admin credentials.

## Remove Admin PIN

Admin PIN feature is removed from the app. It will ask admin credentials for any admin operation required. Admin will be authorized from server.

## Device Diagnostics for GDO

User will have new indications like Cellular Module State and Signal Strength (Air Plane mode and Turn OFF).

## Firmware Upgrade as new SDK 07.02

Latest SDK from Nordic is used for firmware upgrade option.

# Bug Fixes

## Bug # 1890

Sometime user cannot able to open Choose Existing Account screen.

## Bug # 1869

In "SR Device Settings” screen Notification & Auto Connect options are not saved when user turns it off.

## Bug # 1816

Proper alert message should be displayed when invalid response came in web service communication.

## Bug # 1750

Proper validation message should be displayed in configure Keyfob screen.

## Bug # 1721

In Keeler device "Mains" power supply shows as “Alkaline" in "SR Device Settings" screen.

## Bug # 1685

Status bar is not rotating when we perform Lock, Unlock or Status when device is not paired.

## Bug # 1547

Notification functionality is not working properly in mobile with Cellular Data.

# Known Issues and Problems

## Issue # 1

FAQ link is not available from App. Offline FAQ is in Help section of the app.

**Workaround**

Open link for online FAQ - [https://portal.securemote.com/FAQ](https://portal.securemote.com/#/Faq)

## Issue # 2

Sometime even Bluetooth is ON App will display "Turn On BLE” message in "Firmware Upgrade”.

**Workaround**

Turn OFF and again ON your mobile’s Bluetooth from settings. Go to Settings->Bluetooth->OFF and ON

## Issue # 3

User can able to go in "SR Device Settings” screen without pairing with SR device.

**Workaround**

SR Device settings shown in the screen are not actual settings. User needs to press “Save” button to save the actual settings to SR Device.